 

**Approved as an American National Standard**

**ANSI Approval Date: 8/29/2022**

**ANSI/NEMA WC 74/ICEA S-93-639-2022**

*5-46 kV Shielded Power Cable for Use in the   
Transmission and Distribution of Electric Energy*

*Prepared by:*

**Insulated Cable Engineers Association, Inc.**

[www.icea.net](http://www.icea.net/)

*Published by:*

**National Electrical Manufacturers Association**

1300 North 17th Street, Suite 900

Arlington, Virginia 22209

[www.nema.org](http://www.nema.org)

© 2022 National Electrical Manufacturers Association and the Insulated Cable Engineers Association, Inc. All rights including translation into other languages, reserved under the Universal Copyright Convention, the Berne Convention for the Protection of Literary and Artistic Works, and the International and Pan American Copyright Conventions.

**NOTICE AND DISCLAIMER**

The information in this publication was considered technically sound by the consensus of persons engaged in the development and approval of the document at the time it was developed. Consensus does not necessarily mean that there is unanimous agreement among every person participating in the development of this document.

The National Electrical Manufacturers Association (NEMA) and the Insulated Cable Engineers Association (ICEA) standards and guideline publications, of which the document contained herein is one, are developed through a voluntary consensus standards development process. This process brings together persons who have an interest in the topic covered by this publication. While NEMA and ICEA administers the process and establishes rules to promote fairness in the development of consensus, they do not independently test, evaluate, or verify the accuracy or completeness of any information or the soundness of any judgments contained in its standards and guideline publications.

NEMA and ICEA disclaims liability for personal injury, property, or other damages of any nature whatsoever, whether special, indirect, consequential, or compensatory, directly or indirectly resulting from the publication, use of, application, or reliance on this document. NEMA and ICEA disclaims and makes no guaranty or warranty, expressed or implied, as to the accuracy or completeness of any information published herein, and disclaims and makes no warranty that the information in this document will fulfill any of your particular purposes or needs. NEMA and ICEA do not undertake to guarantee the performance of any individual manufacturer or seller’s products or services by virtue of this standard or guide.

In publishing and making this document available, NEMA and ICEA are not undertaking to render professional or other services for or on behalf of any person or entity, nor are NEMA and ICEA undertaking to perform any duty owed by any person or entity to someone else. Anyone using this document should rely on his or her own independent judgment or, as appropriate, seek the advice of a competent professional in determining the exercise of reasonable care in any given circumstances. Information and other standards on the topic covered by this publication may be available from other sources, which the user may wish to consult for additional views or information not covered by this publication.

NEMA and ICEA have no power, nor do they undertake to police or enforce compliance with the contents of this document. NEMA and ICEA do not certify, test, or inspect products, designs, or installations for safety or health purposes. Any certification or other statement of compliance with any health or safety-related information in this document shall not be attributable to NEMA and ICEA and is solely the responsibility of the certifier or maker of the statement.

**Foreword**

This technical publication, *5-46 kV Shielded Power Cable for Use in the Transmission and Distribution of Electric Energy*, was developed by the Insulated Cable Engineers Association, Inc. (ICEA) and approved by the National Electrical Manufacturers Association (NEMA).

ICEA/NEMA standards are adopted in the public interest and are designed to eliminate misunderstandings between the manufacturer and the user and to assist the user in selecting and obtaining the proper product for his particular need. Existence of an ICEA/NEMA standard does not in any respect preclude the manufacture or use of products not conforming to the standard. The user of this standard is cautioned to observe any health or safety regulations and rules relative to the manufacture and use of cable made in conformity with this standard.

Requests for interpretation of this standard must be submitted in writing to:

Insulated Cable Engineers Association, Inc.

[www.icea.net](http://www.icea.net)

An official interpretation will be provided. Suggestions for improvements gained in the use of this standard will be welcomed by the association.

The members of the ICEA working group contributing to the writing of this standard consisted of the following:

Crawford, William, Chairman

Armstrong, John Laughlin, Ed Porter, Kevin

Bodziony, Matt Leblanc, Pierre-Marc Smith, Gregory

Chlebowski, Michael Levitre, Marcel Sorenson, Alex

Davila, Alberto Lindler, Carroll Spradlin, Casey

Filion, Adam Mathew, Abraham Szilagyi, Randy

Fuller, Mark Maximo, Juan Talabathula, Shravani

Ganatra, Ravi Miller, Bruce Temple, Bill

Hammons, Michael Mumm, Jeff West, Tim

Haney, Jacob Nuckles, Kim Weitzel, Jared

Kuchta, Frank Paponetti, Robert Wetzel, Steve

Land, Drayton Perry, Lee

Suggestions for improvement of this standard are welcome. They should be sent to:

National Electrical Manufacturers Association

1300 North 17th Street, Suite 900

Rosslyn, VA 22209

Attention: Secretary ANSI ASC C8

[khaled.masri@nema.org](mailto:khaled.masri@nema.org)

This standard was processed and approved by the Power Control & Instrumentation (PCI) Wire & Cable Subcommittee of the Accredited Standards Committee C8. Subcommittee approval does not necessarily imply that all subcommittee members voted for its approval. At the time it approved this standard, the C8 PCI Subcommittee had the following members:

|  |
| --- |
| Gerald Dorna, Chairman, Belden  Khaled Masri, Secretary, NEMA |
|  |

**Representative Organization**

Kenneth Bow Kable Consult LLC

Lauri Hiivala Power Cable Consultant

Trung Hiu USDA Rural Development Utilities Programs

Michael Kinard Consultant

Anthony Tassone UL LLC

Todd Taylor Enfinity Engineering

William Temple Self—Engineering Consultant

Gerald Dorna Belden

Christel Hunter Cerrowire

Kevin Porter Encore Wire Corporation

Michael Stover Optical Cable Corporation

Henson Toland OFS Fitel

David Watson Southwire Company

Jared Weitzel Prysmian Group

Michael Smalley WEC Energy Group

Ewell Robeson Carolina Power & Light

Contents

Section 1 General 1

1.1 Scope 1

1.2 General Information 1

1.3 Information to Be Supplied by Purchaser 1

1.4 Definitions and Symbols 2

Section 2 Conductor 6

2.1 Physical and Electrical Properties 6

2.2 Optional Water Blocking Components for Stranded Conductors 6

2.3 Conductor Size Units 7

2.4 Conductor DC Resistance Per Unit Length 7

2.5 Conductor Diameter 7

Section 3 Conductor Shield (Stress Control Layer) 14

3.1 Material 14

3.2 Physical Requirements 14

3.3 Electrical Requirements 14

3.4 Crosslinked (Thermoset) Requirements 15

Section 4 Insulation 16

4.1 Material 16

4.2 Insulation Thickness 17

4.3 Insulation Requirements 17

Section 5 Insulation Shielding 23

5.1 Shielding of Insulated Cable 23

5.2 Removability of Insulation Shield 24

Section 6 Metallic Shielding (See Appendix G) 27

6.1 General 27

6.2 Metal Tapes 27

6.3 Copper Wires, Straps, Sheath, or Armor 27

6.4 Multiple-Conductor Cables 28

Section 7 Coverings 29

7.1 Jackets 29

7.2 Metallic and Associated Coverings 35

7.3 Division I 36

7.4 Division II 47

7.5 Division III 50

Section 8 Assembly, Fillers, and Cable Identification 52

8.1 Assembly of Multiple-Conductor Cables 52

8.2 Fillers 53

8.3 Conductor Identification 53

8.4 Cable Identification 53

Section 9 Production Tests and Test Methods 55

9.1 General 55

9.2 Thickness Measurements 58

9.3 Samples and Specimens for Physical and Aging Tests 58

9.4 Aging Tests 61

9.5 Heat Shock Test 61

9.6 Cold-Bend Test 62

9.7 Tightness of Polyethylene Jacket to Sheath Test 62

9.8 Electrical Tests on Completed Cables 62

9.9 Adhesion (Insulation Shield Removability Test) 63

9.10 Hot Creep Test 63

9.11 Solvent Extraction 63

9.12 Wafer Boil Test for Extruded Thermoset Shields 63

9.13 Water Content 63

9.14 Volume Resistivity 64

9.15 Retests 64

9.16 Conductor Test Methods 65

Section 10 Qualification Tests 66

10.1 Accelerated Water Absorption Test 66

10.2 Insulation Resistance Test 66

10.3 Dry Electrical Test for Class III Insulations Only 67

10.4 Test for Discharge-Resistant Insulation (EPR Class IV Insulation Only) 67

10.5 Brittleness Test for Semiconducting Shields 68

10.6 Tray Cable Flame Test 68

10.7 Sunlight Resistance Test 68

10.8 Dielectric Constant and Dissipation Factor 68

10.9 Halogen Content of Nonmetallic Elements 69

10.10 Smoke Generation Test 69

10.11 Acid Gas Equivalent Test 69

10.12 Environmental Stress Cracking Test 69

10.13 Absorption Coefficient 69

10.14 Dielectric Constant and Voltage Withstand for Nonconducting Stress Control Layers 69

Section 11 Constructions of Specific Cable Types 70

11.1 Preassembled Aerial Cable 70

Appendix A Industry Standard References (Normative) 74

Appendix B Emergency Overloads (Normative) 78

Appendix C Procedure for Determining Dimensional Requirements of Jackets and Associated Coverings (Normative) 79

Appendix D Optional Factory DC Test (Informative) 82

Appendix E Representative Tensile Strength and Elongation of Nonmagnetic Metals   
(Informative) 83

Appendix F Voltage Tests During and After Installation (Informative) 84

Appendix G Shielding (Informative) 86

Appendix H Additional Conductor Information (Informative) 88

Appendix I Recommended Bending Radii for Cables (Informative) 91

Appendix J Ethylene Alkene Copolymer (EAM) (Informative) 94

Appendix K Cable Qualification for Submerged Applications (Informative) 95

**Tables**

[Table 2-1 Weight Increment Factors\* 8](#_Toc118224082)

[Table 2-2 Schedule for Establishing Maximum Direct Current Resistance Per Unit Length of   
Completed Cable Conductors Listed in Table 2-4 8](#_Toc118224083)

[Table 2-3 Nominal Direct Current Resistance in Ohms Per 1000 Feet at 25°C of Solid and   
Concentric-Lay-Stranded Conductor 9](#_Toc118224084)

[Table 2-3 (Metric) Nominal Direct Current Resistance in Milliohms Per Meter at 25°C of Solid and Concentric-Lay-Stranded Conductor 10](#_Toc118224085)

[Table 2-4 Nominal Diameters for Copper and Aluminum Conductors 11](#_Toc118224086)

[Table 2-4 (Metric) Nominal Diameters for Copper and Aluminum Conductors 12](#_Toc118224087)

[Table 2-5\*† Factors for Determining Nominal Resistance of Stranded Conductors   
Per 1000 Feet at 25°C 13](#_Toc118224088)

[Table 3-1 Extruded Conductor Shield Physical Requirements 14](#_Toc118224089)

[Table 4-1 Conductor Maximum Rated Temperatures 16](#_Toc118224090)

[Table 4-2 Insulation Physical Requirements 18](#_Toc118224091)

[Table 4-3 Partial Discharge Requirements for Semiconducting Coating and Tape Designs Only 19](#_Toc118224092)

[Table 4-4 Conductor Sizes, Insulation Thicknesses, and Test Voltages 20](#_Toc118224093)

[Table 4-4 (Metric) Conductor Sizes, Insulation Thicknesses, and Test Voltages 21](#_Toc118224094)

[Table 5-1 Requirements for Nonmetallic Conducting Coverings Using Non-Embedded   
Metal Components 24](#_Toc118224095)

[Table 5-2 Requirements for Extruded Nonmetallic Conducting Coverings Using Embedded Metal Components 25](#_Toc118224096)

[Table 5-3 Insulation Shield Thickness Cables Without Embedded Corrugated Wires 25](#_Toc118224097)

[Table 5-4 Insulation Shield Thickness Cables with Embedded Corrugated Wires 26](#_Toc118224098)

[Table 7‑1 Jacket Requirements 32](#_Toc118224099)

[Table 7-2 Low-Smoke, Halogen-Free Jacket Requirements 33](#_Toc118224100)

[Table 7-3 Jacket Irregularity Inspection Test Method 34](#_Toc118224101)

[Table 7-4 Thickness of Overall Jacket of Single- or Multiple-Conductor Cable   
(for All Voltages and All Uses) 34](#_Toc118224102)

[Table 7-5 Thickness of Optional Jacket on Individual Conductors of Multiple-Conductor Cables   
Under a Common Jacket 35](#_Toc118224103)

[Table 7-6 Thickness of Lead Sheath on Unjacketed Cables 37](#_Toc118224104)

[Table 7-7 Thickness of Lead Sheath for Cables Having a Crosslinked or Thermoplastic Jacket   
over Lead Sheath 37](#_Toc118224105)

[Table 7-8 Thickness of Smooth Aluminum Sheath 38](#_Toc118224106)

[Table 7-9 Width of Steel Tape for Flat Armor (Plain or Zinc Coated) 39](#_Toc118224107)

[Table 7-10 Thickness of Steel Tape for Flat Armor (Plain or Zinc Coated) 40](#_Toc118224108)

[Table 7-11 Width of Metal Tape for Interlocked Armor 40](#_Toc118224109)

[Table 7-12 Thickness of Metal Tape for Interlocked Armor 41](#_Toc118224110)

[Table 7-13 Minimum Thickness of Metal for Corrugated Armor 42](#_Toc118224111)

[Table 7-14 Number of Twists (Torsion Test) 43](#_Toc118224112)

[Table 7-15 Minimum Weights of Zinc Coating 43](#_Toc118224113)

[Table 7-16 Mandrel Diameter for Adherence of Coating Tests 43](#_Toc118224114)

[Table 7-17 Size of Galvanized Steel Armor for Submarine Cable 44](#_Toc118224115)

[Table 7-18 Tolerances in Diameter 44](#_Toc118224116)

[Table 7-19 Thickness of Bedding Under Metallic Armor for Unsheathed and Unjacketed Cores 45](#_Toc118224117)

[Table 7-20 Thickness of Servings over Metallic Sheath (Without Metallic Armor) 46](#_Toc118224118)

[Table 7-21 Thickness of Extruded Crosslinked Jackets and Extruded Thermoplastic Jackets   
over Metallic Sheaths and Armors 47](#_Toc118224119)

[Table 7-22 Size of Galvanized Steel Armor Wire for Borehole Cable 48](#_Toc118224120)

[Table 7-23 Spacing and Length of Band Servings 48](#_Toc118224121)

[Table 7-24 Pitch Ratio of Galvanized Wire Armor for Dredge Cable 49](#_Toc118224122)

[Table 7-25 Size of Galvanized Steel Armor Wire for Dredge Cable 49](#_Toc118224123)

[Table 7-26 Size of Galvanized Steel Armor Wire for Shaft Cable and Vertical Riser Cable 50](#_Toc118224124)

[Table 7-27 Thickness of Bedding and Size of Armor Wire (Division III) 51](#_Toc118224125)

[Table 8-1 Conductor Multiplying Factors 52](#_Toc118224126)

[Table 8-2 Grounding Conductor Size 53](#_Toc118224127)

[Table 8-3 Nominal Insulation Thickness 54](#_Toc118224128)

[Table 9-1 Summary of Production Tests and Suggested Sampling Frequency Requirements 56](#_Toc118224129)

[Table 9-2 Mandrel Diameter for Heat Shock Test 61](#_Toc118224130)

[Table 9-3 Mandrel Diameter for Cold-Bend Test 62](#_Toc118224131)

[Table 9-4 Insulation Shield Hot Creep Requirements 63](#_Toc118224132)

[Table 10-1 Accelerated Water Absorption Properties 66](#_Toc118224133)

[Table 10-2 Dielectric Constant and Dissipation Factor 68](#_Toc118224134)

[Table 11-1 Jackets for Type II Preassembled Aerial Cable 71](#_Toc118224135)

[Table 11-2 Messenger Size (Copper-Clad Steel) (ASTM B228 or B229) 72](#_Toc118224136)

[Table 11-3 Messenger Size (ACSR/AW) (ASTM B549) 73](#_Toc118224137)

[Table 11-4 Maximum Tension Limits 73](#_Toc118224138)

[Table D-1 DC Test Voltages 82](#_Toc118224139)

[Table F-1 DC Test Voltages After Installation 85](#_Toc118224140)

[Table H-1 Solid Aluminum and Copper Conductors 88](#_Toc118224141)

[Table H-2 Concentric Stranded Class B Aluminum and Copper Conductors 89](#_Toc118224142)

[Table H-3 Concentric Stranded Class C and D Aluminum and Copper Conductors 90](#_Toc118224143)

[Table I-1 Minimum Radii for Power Cable Single- and Multiple-Conductor Cables with   
Interlocked Armor, Smooth or Corrugated Aluminum Sheath, or Lead Sheath 92](#_Toc118224144)

[Table I‑2 Excerpt from NEMA WC 26‑2008 Wire and Cable Packaging 93](#_Toc118224145)

**< This page left blank intentionally. >**

# Section 1 General

## 1.1 Scope

This standard applies to materials, constructions, and testing of 5,000 volt to 46,000 volt shielded crosslinked polyethylene, and ethylene propylene rubber insulated wires and cables that are used for the transmission and distribution of electrical energy for normal conditions of installation and service, either indoors, outdoors, aerial, underground, or submarine.

Note: See Appendix K for cable insulation qualification requirements or cable design features appropriate for submerged applications.